--lpm_decode CBX_DECLARE_ALL_CONNECTED_PORTS="OFF" DEVICE_FAMILY="MAX 10" LPM_DECODES=2 LPM_WIDTH=1 data eq
--VERSION_BEGIN 15.0 cbx_cycloneii 2015:04:22:18:04:07:SJ cbx_lpm_add_sub 2015:04:22:18:04:07:SJ cbx_lpm_compare 2015:04:22:18:04:07:SJ cbx_lpm_decode 2015:04:22:18:04:08:SJ cbx_mgl 2015:04:22:18:06:50:SJ cbx_stratix 2015:04:22:18:04:08:SJ cbx_stratixii 2015:04:22:18:04:08:SJ  VERSION_END


-- Copyright (C) 1991-2015 Altera Corporation. All rights reserved.
--  Your use of Altera Corporation's design tools, logic functions 
--  and other software and tools, and its AMPP partner logic 
--  functions, and any output files from any of the foregoing 
--  (including device programming or simulation files), and any 
--  associated documentation or information are expressly subject 
--  to the terms and conditions of the Altera Program License 
--  Subscription Agreement, the Altera Quartus II License Agreement,
--  the Altera MegaCore Function License Agreement, or other 
--  applicable license agreement, including, without limitation, 
--  that your use is for the sole purpose of programming logic 
--  devices manufactured by Altera and sold by Altera or its 
--  authorized distributors.  Please refer to the applicable 
--  agreement for further details.



--synthesis_resources = lut 1 
SUBDESIGN decode_2j9
( 
	data[0..0]	:	input;
	eq[1..0]	:	output;
) 
VARIABLE 
	enable	: NODE;
	eq_node[1..0]	: WIRE;

BEGIN 
	enable = VCC;
	eq[] = eq_node[];
	eq_node[] = ( (data[] & enable), ((! data[]) & enable));
END;
--VALID FILE
